1 ;Year must be a 4-digit number higher than 2005.
2 ;Nominal voltage must be a positive decimal number.
3 ;Circuit length of overhead line must be a positive decimal number.
4 ;Circuit length of cable must be a positive decimal number.
5 ;Number of bays in voltage transformation substations/switching stations must be a positive integer.
6 ;Number of secondary distribution substations must be a positive integer.
7 ;Number of house connections must be a positive integer.
8 ;Number of connected end users must be a positive integer.
9 ;Installed rated apparent power of secondary distribution transformers must be a positive decimal number.
10;Installed rated apparent power of end user transformers must be a positive decimal number.
11;For the input of voltage level only values corresponding to index list are allowed.
12;For the input of share of cables in total circuit length only values corresponding to index list are allowed.
13;Identification of network operator must be given.
14;Network operator name must be given.
15;Year must be given.
16;Identification of network must be given.
17;Nominal voltage must be given.
18;Voltage level must be given.
19;Share of cables in total circuit length must be given.
20;For networks with a nominal voltage up to 1 kV number of house connections must be given.
21;For networks with a nominal voltage up to 1 kV number of connected end users must be given.
22;For networks with a nominal voltage above 1 kV at least either installed rated apparent power of secondary distribution transformers or installed rated apparent power of end user transformers must be given.
23;For networks with a nominal voltage up to 1 kV number of bays in voltage transformation substations/switching stations must not be given.
24;For networks with a nominal voltage above 1 kV number of house connections must not be given.
25;For networks with a nominal voltage above 1 kV number of connected end users must not be given.
26;For networks with a nominal voltage up to 1 kV installed rated apparent power of secondary distribution transformers must not be given.
27;For networks with a nominal voltage up to 1 kV installed rated apparent power of end user transformers must not be given.
28;In case of share of cables in total circuit length of overhead line network wiring degree must be lower than 10%.
29;In case of share of cables in total circuit length of mixed networks wiring degree must be between 10 % and 90 %.
30;In case of share of cables in total circuit length of cable networks wiring degree must be higher than 90 %.
31;Identification of network must be explicit within a network data file.
32;Number of LV distributors must be a positive integer.
33;For networks with a nominal voltage up to 1 kV number of LV distributors must be given.
34;For networks with a nominal voltage above 1 kV number of LV distributors must not be given.




